**File handling guide**

**SIGMA: Hydrogen mass flow, its pressure**

Mass flow data were measured by Coriollis flow meter and transmitted to Oscilloscope Sigma

**GEN31: Overpressure**

Overpressure was measured with Kulite XTM - 190-50A pressure transducer and transmitted to Transient Recorder Gen3i HBM.

HTE242USN\_**00004**\_READ190621.mat

Experiment nummer

|  |  |
| --- | --- |
| Mass flow rate and its pressure | Overpressure |
| SIGMA( : , 1 ) – time (s)SIGMA( : , 2 ) – mass flow rate (g/s)SIGMA( : , 3 ) – pressure at the coriolis outlet (bar) | GEN3i( : , 1 ) – time (s)GEN3i( : , 3 ) – overpressure (kPa) |

**Concentration data:**
Concentration data was measured with XENsensors with Labview software.

HTE242USN**00004**CONC190621.xlsx

Experiment nummer

Column B- Time (s)

 C- Concentration (%)

 E- Temperature (°C)